**Ampero II Stomp**

**USB Audio Firmware Update Guide**

Please follow the steps below to update USB Audio firmware:

1. Install USB ASIO Driver (Windows Only)

Please install the **LATEST** Hotone Generic USB ASIO Driver FIRST to ensure all following operations can be done properly. You can download it from our website.

1. Update USB Audio Firmware


Please turn on your Ampero II Stomp **(NORMAL POWER UP, NOT FIRMWARE UPDATE/RESTORE MODE)** and connect to your computer via USB. Then run Hotone USB Audio Device Firmware Updater depending on your OS:

* macOS: Run Hotone Audio USB Audio Device Firmware Updater V1.0.1.pkg contained in Mac Updater folder; after installation, run HOTONEUsbAudioDfu app in Application folder
* Windows: Find and run HOTONEUsbAudioDfu.exe depending on your system type:

32-bit system: Run Windows Updater/x86/HOTONEUsbAudioDfu.exe

64-bit system: Run Windows Updater/x64/HOTONEUsbAudioDfu.exe


Then update USB Audio device firmware following the software’s instructions:



1. *Click Browse button to choose USB audio firmware*
2. *Click Start button to update*

USB Audio firmware is a .bin file included in root folder of this zip file.

When update progress finished, a “Firmware upgrade finished successfully.” Message will come up in the message box shown as below:

**

*Please notice firmware version change after firmware update*

Click Exit button to finish USB Audio firmware update.